( TL19E00J10300000000FAAT05 )

Audio System Symptom Troubleshooting - No sound is heard from the speaker(s) (display is normal) (with premium audio system)

1. Check for continuity between audio unit connector A (24P), connector C (12P), and stereo amplifier connector B (28P) according to the table.

   Audio unit connector | Stereo amplifier terminal
   --- | ---
   A17 (WHT) | B3 (YEL)
   A18 (GRN) | B25 (RED)
   A19 (BLK) | B11 (GRN)
   A21 (GRY) | B12 (GRY)
   A22 (WHT) | B24 (WHT)
   A23 (RED) | B10 (BLK)
   C1 (RED) | B1 (RED)
   C2 (GRN) | B15 (GRN)
   C7 (GRY) | B16 (GRY)

Is there continuity?

YES | - | Go to Step 23 .
NO | - | Repair open in the applicable wire(s) between the audio unit and stereo amplifier.■