( TL19E00K7090008A120FAAT00 )

DTC Troubleshooting: 112

1. Check for continuity between the ACC unit 20P connector No. 20 terminal and the VSA modulator-control unit 47P connector No. 13 terminal.

Is there continuity?

YES | - | Check for loose or poor connections. If the connections are OK, update the ACC unit, then recheck. If the ACC unit was already updated, replace the ACC unit. ■
NO | - | Repair an open in the wire between the ACC unit and the branch of the F-CAN line (CANL).■