( TL19E00K773000Y1825FAAT00 )

DTC Troubleshooting: B1825

1. Check for continuity between body ground and slide motor/position sensor 5P connector No. 1 and No. 5 terminals individually.

Is there continuity?

YES | - | Repair a short to ground in the wire.■
NO | - | Go to Step 31 .

1. Test the slide motor.

Is the motor OK?

YES | - | Replace the power seat control unit .■
NO | - | Replace the slide motor/position sensor.■

LHD model
RHD model