( TL19E00D14300014751KBAT00 )

Brake Hose Replacement

NOTE:

- Before reassembling, check that all parts are free of dirt and other foreign particles.
- Replace parts with new ones whenever specified to do so.
- Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid gets on the paint, wash it off immediately with water.
- Plug the end of a hose and joints to prevent spilling brake fluid.

Front
NOTE: The illustrations show the 1-piston caliper type.

1. Remove the front wheel.

1. Disconnect the brake line (A) from the brake hose (B), then remove the brake hose clip (C).

1. Remove the banjo bolt (A), and disconnect the brake hose (B) from the caliper.

1. Remove the brake hose mounting bolt (C), then remove the brake hose.

1. Install the brake hose (A) with the mounting bolt (B).

1. Connect the brake hose to the caliper with the banjo bolt (C) and the new sealing washers (D).

1. Install a new brake hose clip (A) to the brake hose (B) on the bracket, then connect the brake line (C). Do not twist the brake hose.

1. After installing the brake hose, bleed the brake system.

1. Do the following checks:
   - Check the brake hose and line joint for leaks, and tighten if necessary.
   - Check the brake hoses for interference and twisting.

1. Clean the mating surfaces of the brake disc and the inside of the wheel, then install the front wheel.

Rear
NOTE: The illustrations show the rear disc brake type.

1. Remove the rear wheel.

1. Disconnect the brake line (A) from the brake hose (B), then remove the brake hose clip (C).

1. Remove the banjo bolt (A), and disconnect the brake hose from the caliper.

1. Remove the brake hose mounting bolt (B), then remove the brake hose.

1. Install the brake hose (A) with the mounting bolt (B).

1. Connect the brake hose to the caliper with the banjo bolt (C) and new sealing washers (D).

1. Install a new brake hose clip (A) to the brake hose (B) on the bracket, then connect the brake line (C). Do not twist the brake hose.

1. After installing the brake hoses, bleed the brake system.

1. Do the following checks:
   - Check the brake hose and line joint for leaks, and tighten if necessary.
   - Check the brake hose for interference and twisting.

1. Clean the mating surfaces of the brake disc and the inside of the wheel, then install the rear wheel.