( TL19E00J26273450001KDAT00 )

Interior Trim Removal/Installation - Rear Shelf Area

Rear Parcel Shelf Dynamic Damper - With Premium Sound System
NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the body.

1. Remove the rear shelf.

1. Remove the bolts, then remove the rear parcel shelf dynamic damper (A). Take care not to hit the rear window when removing the bolts.

1. Install the damper in the reverse order of removal.