( TL19E00J10300000000FAAT01 )

Audio System Symptom Troubleshooting - Poor AM or FM radio reception or interference (with premium audio system)

1. Check for continuity between the audio unit connector E (5P) terminal No. 5 and the AM/FM antenna 3P connector terminal No. 3.

Is there continuity?

YES | - | Go to Step 14 .
NO | - | Repair open in the wire between the audio unit and the AM/FM antenna. Also check the AM/FM antenna lead/sublead connector.■