( TL19E00H46400000000CAAT00 )

E-pretensioner
The mechanical portion of the E-pretensioner consists of the motor and the gear sections. When the collision mitigation brake or the brake assist system signals are input, the motor in the retractor section is driven to rewind or retract. If the system judges that the driving situation is safe, the tension on the seat belts is released. The E-pretensioners used in conjunction with the conventional tensioners.