( TL19E00J46127053632KBAT00 )

Front Seat Cushion Cover Replacement

SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Put on gloves to protect your hands.
- Take care not to tear the seams of damage the seat covers.
- When removing components, use the trim tools or equivalent.
- LHD model is shown, RHD model is symmetrical.

1. Remove the front seat.

1. 8-way power seat: Remove the screw, and release the hooks (A), the tabs (B), and the pin (C), then remove the front cover (D). The driver's seat is shown; the passenger's seat is symmetrical.