( TL19E00J46643436101FEAT00 )

Keyless Entry Transmitter Test

1. Replace the transmitter battery (A) with a new one, and try to lock and unlock the doors with the transmitter by pressing the lock or unlock button five or six times.
   - If the doors lock and unlock, the transmitter is OK.
   - If the doors don't lock and unlock, go to Step 5 .

1. Reprogram and register the transmitter, then try to lock and unlock the doors.
   - If the doors lock and unlock, the transmitter is OK.
   - If the doors don't lock and unlock, substitute a known-good transmitter and recheck. If still not operating, replace the immobilizer-keyless control unit.
   NOTE: As the keyless transmitter is combined with the immobilizer transponder, so when the transponder is registered by the HDS, the keyless transmitter is also registered automatically.