( TL19E00J10300000000CAAT10 )

Audio/Navigation Switch Panel for Inputs and Outputs (With Navigation System)
Audio/Navigation Switch Panel 24P Connector

Cavity | Wire | Connects to
--- | --- | ---
1 | WHT | Audio unit (ENC−)
3 | BLU | Audio unit (DUET CONT)
6 | GRN | Audio unit (OPERA TX)
7 | RED | Climate control unit (DISP CLK)
10 | BLK | Ground (G401) (GND)
11 | ORN | Dashlight brightness controller (ILL−LED)
12 | RED | Dashlight brightness controller (ILL−BULB)
13 | BLK | Audio unit (ENC+)
14 | ORN | Audio unit (PWR SW)
15 | GRN | Audio unit (DUET RX (UART))
16 | RED | Audio unit (DUET TX (UART))
17 | BRN | Audio unit (OPERA CONT)
18 | RED | Audio unit (OPERA RX)
19 | PUR | Climate control unit (DISP SI)
21 | LT GRN | Audio/navigation switch panel power supply (IG2)
22 | WHT | Constant power (+B)
23 | GRY | Light-on signal (ILL+)