( TL19E00J46127053949KBAT00 )

Front Seat-back Cover Replacement

1. Passenger's seat with OPDS: Remove the OPDS unit cover (A).

   -1. | Turn over the seat-back cover (B) and pad (C) as needed.
   -2. | Release the cover from the lower hooks (D).
   -3. | Pull the cover upward to release it from the upper hook (E).

1. Passenger's seat with OPDS: Disconnect the OPDS unit harness connector (F) and the OPDS sensor connectors (G).