( TL19E00J46166453984KDAT00 )

Rear Seat-back Latch/Release Cable Removal/Installation

NOTE:

- Take care not to bend or scratch the interior trim.
- The left rear seat-back latch/release cable is shown; the right rear seat-back latch/release cable is similar.

1. Remove the rear seat-back release lever.

1. From the trunk compartment, detach the cable clip fastening the seat-back release cable (A).

1. Remove the rear bulkhead cover.