( TL19E00J26220219281KDAT00 )

Dashboard Center Lower Cover Removal/Installation

1. Remove the passenger's dashboard center lower cover (A).

   -1. | Gently pull the rear edge of the cover to detach the clip (B), and detach the farther clip (C) at the front of the cover.
   -2. | Pull up the cover to release the hook (D) from the rear heater duct (E).

1. Install the cover in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.
   - Make sure the hooks are set properly.