( TL19E1RE10436455079KBAT00 )

A/T Interlock System - Shift Lock Release, Release Spring, and Release Extension Replacement

NOTE: This replacement applies for the RHD model.

1. Remove the shift lever assembly.

1. Remove the shift lever knob.

1. Remove the shift lever boot and the A/T gear position indicator panel base.

1. Release the lock (A) of the shift lock release extension (B), and remove the shift lock release extension.

1. Push the stop lever (C) of the shift lock release (D), and remove the shift lock release.