( TL19E00H46400012831KBAT00 )

Front Passenger's Airbag Off Indicator Replacement

1. With navigation: Remove the navigation display unit.

1. Without navigation: Remove the center display unit.

1. Disconnect the 4P connector (A) from the passenger's airbag off indicator (B).

1. Remove the screw (C), then pull out the passenger's airbag off indicator from the navigation display unit (with navigation) or the center display unit (without navigation).

1. Reinstall the parts in the reverse order of removal.