( TL19E1PE10411619631KBAT00 )

A/T Differential Oil Seal Replacement

Special Tools Required
Driver handle 15 x 135L
07749-0010000
Oil seal driver attachment
07947-SD90101
Oil seal driver attachment 58
07JAD-PH80101
NOTE: Be careful not damage the transmission housing and the torque converter housing while removing the oil seals.

1. Remove the oil seal from the transmission housing.

1. Remove the oil seal from the torque converter housing.

1. Install a new oil seal (A) in the transmission housing using the 15 x 135L driver handle and oil seal driver attachment 58.

1. Install a new oil seal (A) in the torque converter housing using the 15 x 135L driver handle and oil seal driver attachment 58.