( TL19E00J10300000000FAAT13 )

Audio System Symptom Troubleshooting - Audio disc changer does not move between discs

Audio disc changer does not move between discs
NOTE:

- Check the vehicle battery condition first.
- Check the connectors for poor connections or loose terminals.
- Disc labels should not be used in the audio unit. They may damage the player mechanism.

1. Turn the ignition switch to ON (II).

1. Insert six discs into the audio unit (in-dash disc changer) and see if the changer moves between discs.

Does the changer operate normally?

YES | - | Intermittent failure, the disc changer is OK at this time.■
NO | - | Go to Step 3 .

1. Insert six known-good discs into the audio unit.

Does the changer operate normally?

YES | - | At least one of the original discs is faulty.■
NO | - | Substitute a known-good audio unit (in-dash disc changer) with navigation system , without navigation system , and recheck. If the symptom/indication goes away, replace the original audio unit (in-dash disc changer) with navigation system , without navigation system. ■