( TL19E00J46166400000KDAT00 )

Rear Seat Removal/Installation

1. Lift the seat side bolster (A) up to release the hooks (B), then remove the seat side bolster.

1. Install the seat side bolster in the reverse order of removal, and note these items:
   - Guide the belts over the front of the seat side bolster as you install the bolster.
   - Before attaching the seat side bolster, make sure there are no twists or kinks in the seat belts.