( TL19E00D14300014711LAAT10 )

Front Brake Caliper Overhaul

1. Mount the commercially available brake caliper piston compressor tool (A) on the caliper body (B).

1. Press in the piston with the brake caliper piston compressor tool. Make sure that the piston boot is properly positioned into the groove of the piston.
   NOTE:
   - Do not press the piston diagonally, and do not press it forcibly.
   - Be careful not to damage the piston boot when press the piston.

1. Install the caliper body.