( TL19E00J22100030053BBAT00 )

Gauge Control Module Self-diagnostic Function

The Indicator Drive Circuit Check When entering the self-diagnostic mode, the following indicators blink: A/T gear position indicator, ABS indicator, brake system indicator, charging system indicator, cruise control indicator, cruise main indicator, high beam indicator, immobilizer indicator, lights-on indicator, low oil pressure indicator, low fuel indicator, low oil pressure indicator, malfunction indicator lamp (MIL), seat belt indicator, security indicator, side airbag cutoff indicator, SRS indicator, VSA activation indicator, VSA indicator, EPS indicator, M/T shift up indicator, M/T shift down indicator, turn signal indicator, front fog light indicator, rear fog light indicator, CMBS indicator, LKAS indicators, ACC indicators, and message indicator. |