( TL19E1AE34100000000HAAT01 )

Hard to shift into 1st gear

Probable cause(s)

1. Worn or incorrect MTF.
2. Clutch defective.
3. 1st synchro ring defective.
4. 1st/2nd synchro sleeve and hub defective.
5. 1st gear defective.
6. Change lever assembly defective.

Diagnostic procedure

- Check and/or replace the MTF.
- Check the clutch.
- Check the 1st synchro ring.
- Check the 1st/2nd synchro sleeve and hub.
- Check 1st gear.
- Check the change lever assembly.