( TL19E00J26220200000KBAT00 )

Dashboard Replacement

1. While holding the dashboard (A) away from the body, detach the antenna sublead clip (B) from the passenger's side bracket (C). Pull the antenna sublead (D) out from under the dashboard wire harness (E).

1. Carefully remove the dashboard through the front door opening.
   NOTE: Do not rest the dashboard on its lower center cover opening, or it may be damaged. Lay it on its front or back.