( TL19E00G24113600000KDAT00 )

Blower Unit Removal/Installation

1. Remove the passenger's dashboard undercover.

1. Remove the passenger's dashboard trim.

1. Remove the glove box.

1. Remove the passenger's dashboard center lower cover.

1. Remove the bolts (A) and the connector clips (B). Then cut the plastic cross brace (C) in the glove box opening with diagonal cutters in the area shown. Retain plastic cross brace to be reinstalled later.