( TL19E00J36100000000CAAT20 )

Navigation Unit Inputs and Outputs
Navigation Unit Connector E (2P)

Terminal Number | Wire Color | Terminal Name | Description | Voltage (about) | Symptom
--- | --- | --- | --- | --- | ---
1 | ——— | SIG (GPS) | GPS signal | 5 V | If open: GPS icon is not shown, system links screen ANT shows NG. If short to body ground: Same as open.
2 | ——— | SH (GPS) | Ground for GPS signal | 0 V | If open: GPS icon is not shown, system links screen ANT shows NG. If short to body ground: No effect on system.