( TL19E00J18513415017KBAT00 )

Front Bumper Lower Grille Replacement

1. With headlight washer: Release the washer tube (A) from the holders (B) of the front bumper lower grille (C). Detach the hooks (D, E), then remove the lower grille from the front bumper (F).

1. Install the bumper lower grille in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips and the hooks into place securely.