( TL19E00J10300013151KDAT01 )

Audio Unit Removal/Installation - With NAV.

With Navigation System
SRS components are located in this area. Review the SRS component locations, and the precautions and procedures before doing repairs or service.
NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the dashboard and related parts.
- Lay a workshop towel under the parts when working on them to protect the face panel from scratches or other damage.
- Eject all the disc before remove the audio unit to prevent damaging the CD/DVD player's load mechanism.
- If you are replacing the audio unit, write down the audio presets (if possible), then enter them into the new audio unit.

1. Remove these items:
   - Driver's center trim
   - Passenger's dashboard trim
   - Passenger's center trim
   - Center console panel
   - Climate control unit

1. Make sure you have the anti-theft code for the audio system and the navigation system.

1. Remove the bolts, then pull out the audio unit (A).

1. Disconnect the connectors (B), then remove the audio unit.

1. Install the audio unit in the reverse order of removal, and note these items:
   - Make sure all the connectors and the antenna lead are secure.
   - Enter the anti-theft codes for the audio system.
   - If necessary, enter the navigation system code (KQ model).

1. Give the new anti-theft codes to the customer.