( TL19E00J4616185367CKBAT00 )

Front Seat Up-down Motor Motor Replacement

Rear Up-down Motor - 8-Way Power Seat
NOTE:

- Put on gloves to protect your hands.
- The driver's seat on LHD model is shown; the passenger's seat is symmetrical; the ones on RHD model are similar.

Removal

1. Remove the front seat.

1. Remove these items:
   - Seat-back cover/pad
   - Seat cushion cover/pad

1. Remove the rear brake (A) and the rear brake bracket (B) as an assembly.

   -1. | Using a TORX T30 bit, remove the brake bracket mounting bolts (C).
   -2. | Using a TORX T40 bit, remove the brake bracket mounting bolt (D).
   -3. | Pull the brake bracket back to remove the gear (E) from the brake gear axle.