( TL19E00J10300000000FAAT02 )

Audio System Symptom Troubleshooting - Poor AM or FM radio reception or interference (without premium audio system)

1. Check for continuity between the audio unit connector E (3P) terminal No. 3 and body ground.

Is there continuity?

YES | - | Repair short to body ground in the wire between the audio unit and AM/FM antenna.■
NO | - | Replace the audio unit. ■

1. Remove the audio unit.

1. Disconnect audio unit connector E (3P).