( TL19E00F18100000000CAAT00 )

Motion Adaptive EPS System Outline
The EPS and VSA compensate for bad handling and instability caused by adverse weather conditions such as rain, snow, or crosswind.
This system is composed of the EPS control unit, the torque sensor, the VSA modulator-control unit, the wheel speed sensors, the steering angle sensor, the yaw rate-lateral acceleration sensor, and the system indicators in the gauge control module.