( TL19E00J36100000000FAAT20 )

Navigation System Symptom Troubleshooting - Rearview camera does not come on or work properly

1. Check for continuity between navigation display unit 28P connector and body ground according to the table. Then check for continuity between navigation display unit 28P connector No. 11 terminal, rearview camera 6P connector No. 5 terminal and the same terminals.

   Navigation display unit connector | Wire color
   --- | ---
   No. 12 | RED
   No. 13 | WHT
   No. 26 | GRN
   No. 27 | BLK
   No. 28 | BRN

Is there continuity?

YES | - | Repair short in the wire between navigation display unit and the rearview camera, or replace the appropriate shielded harness.■
NO | - | Go to Step 7 .