( TL19E1PE10410412270KDAT00 )

A/T Housing Reverse Idler Gear Removal and Installation

Installation

1. Install the reverse idler gear in the transmission housing.

1. Lightly coat the reverse idler gear shaft (A), needle bearing (B), and new O-rings (C) with lithium grease.

1. Assemble new O-rings and the needle bearing on the reverse idler gear shaft, then install the reverse idler gear shaft in the reverse idler gear shaft holder (D). Align the D-shaped cut out (E) of the reverse idler gear shaft with the D-shaped area (F) of the reverse idler gear shaft holder.