( TL19E00J20170700000KBAT00 )

Subframe Replacement

Rear Subframe Torque
NOTE:

- When installing, align both installation reference holes in the subframe with the reference holes in the body using the subframe alignment pin, and align both installation holes in the rear subframe mounting front stays with the reference holes in the body using the subframe alignment pin.
- After removing the subframe mounting bolts, be sure to replace them with new ones.