( TL19E1QE10436445401KBAT00 )

A/T Interlock System - Park Pin Switch/Shift Lock Solenoid Harness Replacement

LHD model
NOTE: The A/T gear position indicator panel light, the park pin switch, and the shift lock solenoid harness are not available separately. Replace the A/T gear position indicator panel light, the park pin switch, and the shift lock solenoid harness as a set.

1. Remove the shift lever assembly.

1. Remove the shift lever knob.

1. Remove the A/T gear position indicator panel base.

1. Release the lock (A) of the shift lock release (B), then remove the shift lock release and the release spring (C).

1. Remove the shift lock solenoid.