( TL19E1PE10400000000HAAT20 )

Poor acceleration; stall speed low in D and S in 1st and 2nd

Probable Cause(s)

1. Shift solenoid valve E defective
2. Torque converter one-way clutch defective
3. Engine output low
4. Torque converter clutch piston defective
5. Lock-up shift valve defective

Notes

- Check for a stored DTC, and check for loose connectors.
- Inspect shift solenoid valve E for seizure, and the O-rings for wear and damage.
- Replace the torque converter.