( TL19E00K783000Y1302FAAT00 )

DTC Troubleshooting: B1302

DTC B1302:
Rain Sensor (EEPROM) Error

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Wait for 6 seconds or more.

1. Check for DTCs with the HDS.

Is DTC B1302 indicated?

YES | - | Replace the automatic lighting/ rain sensor .■
NO | - | Intermittent failure, the automatic lighting/ rain sensor is OK at this time.■