( TL19E00J18513415045KBAT00 )

Front Bumper Spoiler Replacement

For Some Models
NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the front bumper.

1. Remove the screws (A) securing the front bumper (B) and the front bumper spoiler (C) from both wheel arch portions.

1. Remove the bolts (D, E) securing the bumper and the spoiler from under the bumper.

1. Pull the front bumper spoiler back along the edge of it near the double-sided adhesive tape (F) and the double-sided adhesive tape (G) of the spoiler spacers (H) to release them from the front bumper, then remove the spoiler.