( TL19E00K761000N1303FAAT00 )

DTC Troubleshooting: 1303

DTC 1303:
GPS Receiver Error 2
NOTE:

- Check the vehicle battery condition first.
- Before you troubleshoot, make sure to follow the general troubleshooting information.
- Make sure the vehicle is parked outside and away from buildings.
- Aftermarket electronic devices located near the navigation unit or GPS antenna can potentially interfere with the operation of the navigation system.

1. Clear the hard error code.

1. Turn the ignition switch to LOCK (0), and then back to ON (II).

1. Check for the hard error code.

Is DTC 1303 indicated?

YES | - | Replace the navigation unit. ■
NO | - | Intermittent failure, the system is OK at this time.■