( TL19E1PE10410744858KBAT00 )

A/T Paddle Shifter + (Upshift Switch) Replacement

SRS components are located in this area. Review the SRS component locations and the precautions and procedures in the SRS before doing repair or service.

1. Remove the steering wheel.

1. Remove the two screws (A) securing the steering wheel rear cover (B).

1. Release the locks (C) of the steering wheel rear cover, and remove the steering wheel rear cover.

1. Remove the four screws (D) securing the steering wheel trim (E).

1. Release the hook (F) and pull up the pins (G) by pulling the steering wheel trim.

1. Disconnect the connectors (H) from the steering wheel trim.