( TL19E2PK7710009060AFAAT00 )

DTC Troubleshooting: P060A (131)

DTC P060A:
PCM (A/T system) Internal Control Module Malfunction
NOTE: Before you troubleshoot, record all freeze data and any on-board snapshot, and review the general troubleshooting information.

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P060A indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Update the PCM if it does not have the latest software, or substitute a known-good PCM.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P060A indicated?

YES | - | If the PCM was updated, substitute a known-good PCM, then recheck. If the PCM was substituted, go to Step 1 .
NO | - | If the PCM was updated, troubleshooting is complete. If the PCM was substituted, replace the original PCM. If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.■