( TL19E00D00060800000MCAT00 )

Parking Brake Inspection and Adjustment

1. Remove the access plug (A).

1. Turn the ratchet teeth (B) on the adjuster assembly (C) with a flat-tip screwdriver (D) until the shoes lock against the parking brake drum. Then back off the adjuster 8 clicks, and install the access plug.

1. Do the minor adjustment procedure.

1. Clean the mating surfaces of the brake disc/drum and the inside of the wheel, then install the rear wheels.

1. Close the lid, then install the console box mat.