( TL19E00J54200000000BBAT00 )

How to Troubleshoot the Body Electrical

HDS Inputs and Commands
Input:

System Menu | Data List | Data List Indication
--- | --- | ---
Keyless | Driver's Door Key Cylinder Switch (LOCK) | OFF/ON
Driver's Door Key Cylinder Switch (UNLOCK) | OFF/ON
Driver's Door Lock Switch (LOCK) | OFF/ON
Driver's Door Lock Switch (UNLOCK) | OFF/ON
Driver's Door Lock Knob Switch (LOCK) | OFF/ON
Driver's Door Lock Knob Switch (UNLOCK) | OFF/ON
Driver's Door Switch | OFF/ON
Driver's Rear Door Switch | OFF/ON
Trunk Lid/Tailgate Switch | OFF/ON
Driver's Rear Door Lock Knob Switch (UNLOCK) | OFF/ON
Door LOCK Command | OFF/ON
Door UNLOCK Command | OFF/ON
Driver's Door UNLOCK Command | OFF/ON
Trunk Lid Release Command | OFF/ON
Front Passenger's Door Switch | OFF/ON
Passenger's Rear Door Switch | OFF/ON
Passenger's Rear Door Lock Knob Sw. (UNLOCK) | OFF/ON
Door LOCK Command | OFF/ON
Door UNLOCK Command | OFF/ON
Power Windows | P/W Main Switch | OFF/ON
P/W Master Switch (Driver's Window AUTO) | OFF/ON
P/W Master Switch (Driver's Window UP) | OFF/ON
P/W Master Switch (Driver's Window DOWN) | OFF/ON
P/W Master Sw. (Front Passenger's Window UP) | OFF/ON
P/W Master Sw. (Front Passenger's Window DOWN) | OFF/ON
P/W Master Switch (Left Rear Window UP) | OFF/ON
P/W Master Switch (Left Rear Window DOWN) | OFF/ON
P/W Master Sw. (Right Rear Window UP) | OFF/ON
P/W Master Sw. (Right Rear Window DOWN) | OFF/ON
P/W Master Sw. (Passenger's Window AUTO) | OFF/ON
Driver's P/W Motor Pulse A | NOT EXIST/EXIST
Driver's P/W Motor Pulse B | NOT EXIST/EXIST
Driver's P/W Motor Command | OFF/UP/DOWN
Driver's Door Switch | OFF/ON
Power Window Timer Output | OFF/ON
Front Passenger's Door Switch | OFF/ON
Power Window Timer Output | OFF/ON