( TL19E00J36100000000FEAT00 )

Navigation System Diagnostic Mode

TMC Status (KG and KE models)
This screen displays a state about the RDS-TMC reception.
Frequency: Frequency receiving in this time.
Field Strength: Display reception sensitivity with 0−15.
0−5: Cannot receive
6: Instability
7−8: Can receive it somehow
9−15: Can receive it clear
Error Rate Correction: RDS block error.
0: No error
1: Synchronous error
2: Block number error
Others: Undefined
Uncorrected Block/min: The number of block errors per one minute.
TMC Group Counter: The number of message which l received.
Provider Count: The number of providers which l can receive.