DTC B2741 [DSC]

#
DTC B2741 [DSC]

B3E040243000W15

DTC | B2741 | Combined sensor (internal malfunction)
DETECTION CONDITION | • Combined sensor internal malfunction is detected.
POSSIBLE CAUSE | • Combined sensor internal malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY COMBINED SENSOR MALFUNCTION • Clear the DTCs from the memory. (See Clearing DTCs Procedures.) • Are the same DTCs present? | Yes | Replace the combined sensor, then go to the next step. (See COMBINED SENSOR REMOVAL/INSTALLATION.)
No | Go to the next step.
2 | VERIFY THAT NO OTHER DTCS ARE PRESENT • Are any other DTCs output? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | DTC troubleshooting completed.