NO.1 MELTING OF MAIN OR OTHER FUSES [ZJ, Z6]

#
NO.1 MELTING OF MAIN OR OTHER FUSES [ZJ, Z6]

B3E010318881W34

1 | MELTING OF MAIN OR OTHER FUSES
--- | ---
[TROUBLESHOOTING HINTS] Inspect condition of fuse.

Damaged fuse | Related wiring harness
--- | ---

IG KEY1
(30 A)

IG KEY1 fuse

• Ignition switch

  - ENGINE fuse

ENGINE (20 A) | ENGINE fuse • Main relay

IG KEY2
(30 A)

IG KEY2 fuse

• Ignition switch

  - BACK fuse

BACK (10 A) | BACK fuse • TR switch
ENG +B (10 A) | ENG +B • PCM

ENGINE
(30 A)

ENGINE fuse

• Main relay

  - EGI INJ1 fuse
  - EGI INJ2 fuse
  - EGI BAR1 fuse

EGI INJ1 (10 A) | EGI INJ1 fuse • PCM
EGI INJ2 (10 A) | EGI INJ2 fuse • PCM
ENG BAR1 (10 A) | ENG BAR1 fuse • PCM • Fuel pump relay
FUEL PUMP (15 A) | FUEL PUMP fuse • Fuel pump relay
FAN (40 A) | FAN fuse • FAN control module
BTN (40 A) | BTN fuse • OBD fuse
OBD (10 A) | OBD fuse • DLC-2