SYMPTOM TROUBLESHOOTING CHART

#
SYMPTOM TROUBLESHOOTING CHART

B3E090369000W04

No. | Troubleshooting item | Description
--- | --- | ---
1 | One or more on-board diagnostic functions inoperative | • Malfunction in door lock linkage system
2 | All on-board diagnostic functions inoperative | • Malfunction in PJB power supply circuit, door latch switch circuit, PJB ground circuit, or keyless control module.
3 | Transmitter ID code cannot be reprogrammed | • Malfunction in transmitter battery, transmitter, keyless receive bracket, keyless receive bracket ground screw, or PJB circuit. keyless receive circuit.