DTC B1342

#
DTC B1342

B3E060201038W05

DTC | B1342 | EHPAS control module
DETECTION CONDITION | • The EHPAS control module on-board diagnostic function detects system malfunction.
POSSIBLE CAUSE | • EHPAS control module internal malfunction • Poor connection at connectors

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY THAT THE SAME DTC IS NOT PRESENT • Clear the DTC from the memory. (See Clearing DTCs Procedure.) • Is the same DTC present? | Yes | Replace the electric power steering oil pump, then go to the next step. (See ELECTRIC POWER STEERING OIL PUMP (LF) REMOVAL/INSTALLATION.)
No | Go to the next step.
2 | VERIFY THAT NO OTHER DTCS ARE PRESENT • Are any other DTCs output? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | DTC troubleshooting completed.