CAR-NAVIGATION UNIT REMOVAL/INSTALLATION

#
CAR-NAVIGATION UNIT REMOVAL/INSTALLATION

B3E092066902W01

1. Disconnect the negative battery cable.

2. Remove the decoration panel.(See DECORATION PANEL REMOVAL/INSTALLATION.)

3. Remove the front scuff plate.(See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

4. Remove the front side trim.(See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

5. Remove the glove compartment.(See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

1 | Nut
2 | Connector
3 | Car-navigation unit

7. Install in the reverse order of removal.