CHILD-RESTRAINT SEAT ANCHOR REMOVAL/INSTALLATION

#
CHILD-RESTRAINT SEAT ANCHOR REMOVAL/INSTALLATION

B3E081100117W01

## 4SD

1. Remove in the order indicated in the table.

.

1 | Cover
2 | Bolt
3 | Child-restraint seat anchor

2. Install in the reverse order of removal.

## 5HB

1. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

.

1 | Bolt
2 | Child-restraint seat anchor

3. Install in the reverse order of removal.