REAR STABILIZER REMOVAL/INSTALLATION

#
REAR STABILIZER REMOVAL/INSTALLATION

B3E021428100W01

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

.

1 | Rear crossmember bracket
2 | Rear stabilizer component (See Rear Stabilizer Component Installation Note.)
3 | Stabilizer control link
4 | Stabilizer bracket (See Stabilizer Bracket Removal Note.) (See Stabilizer Bracket Installation Note.)
5 | Stabilizer bushing (See Stabilizer Bushing Installation Note.)
6 | Rear stabilizer

## Stabilizer Bracket Removal Note

1. Secure the stabilizer bracket flange using a vise.

2. Remove the stabilizer bracket.

## Stabilizer Bushing Installation Note

1. Place the stabilizer bushing so that the projection is facing toward the left side of the vehicle.

2. Widen the stabilizer bushing opening 16-26 mm {0.7-1.0 in} and install the bushing to the rear stabilizer as shown in the figure.

## Stabilizer Bracket Installation Note

1. Apply grease to the stabilizer bushing.

2. Install the stabilizer bracket using a vise.

## Rear Stabilizer Component Installation Note

1. Tighten the bolts in order indicated in the figure.