HVAC CONTROL SYSTEM LOCATION INDEX [FULL-AUTO AIR CONDITIONER]

#
HVAC CONTROL SYSTEM LOCATION INDEX [FULL-AUTO AIR CONDITIONER]

B3E074001042W01

L.H.D.

R.H.D.

.

1 | Air intake actuator (See AIR INTAKE ACTUATOR REMOVAL/INSTALLATION.) (See AIR INTAKE ACTUATOR INSPECTION.)
2 | Air mix actuator (See AIR MIX ACTUATOR REMOVAL/INSTALLATION.) (See AIR MIX ACTUATOR INSPECTION.)
3 | Airflow mode actuator (See AIRFLOW MODE ACTUATOR REMOVAL/INSTALLATION.) (See AIRFLOW MODE ACTUATOR INSPECTION.)
4 | Blower motor (See BLOWER MOTOR REMOVAL.) (See BLOWER MOTOR INSTALLATION.) (See BLOWER MOTOR INSPECTION.)
5 | Power MOS FET (See POWER MOS FET REMOVAL/INSTALLATION.) (See POWER MOS FET INSPECTION.)
6 | Magnetic clutch (Z6, ZJ) (See MAGNETIC CLUTCH DISASSEMBLY/ASSEMBLY [Z6, ZJ].) (See MAGNETIC CLUTCH ADJUSTMENT.) (See MAGNETIC CLUTCH INSPECTION [Z6, ZJ].)
7 | Magnetic clutch (LF) (See MAGNETIC CLUTCH DISASSEMBLY/ASSEMBLY [LF].) (See MAGNETIC CLUTCH ADJUSTMENT.) (See MAGNETIC CLUTCH INSPECTION [LF].)
8 | Solar radiation sensor (See SOLAR RADIATION SENSOR REMOVAL/INSTALLATION.) (See SOLAR RADIATION SENSOR INSPECTION.)
9 | Ambient temperature sensor (See AMBIENT TEMPERATURE SENSOR REMOVAL/INSTALLATION.) (See AMBIENT TEMPERATURE SENSOR INSPECTION.)
10 | Cabin temperature sensor (See CABIN TEMPERATURE SENSOR REMOVAL/INSTALLATION.) (See CABIN TEMPERATURE SENSOR INSPECTION.)
11 | Evaporator temperature sensor (See EVAPORATOR TEMPERATURE SENSOR REMOVAL/INSTALLATION.) (See EVAPORATOR TEMPERATURE SENSOR INSPECTION.)
12 | Refrigerant pressure switch (See REFRIGERANT PRESSURE SWITCH REMOVAL/INSTALLATION.) (See REFRIGERANT PRESSURE SWITCH INSPECTION.)
13 | Climate control unit (See CLIMATE CONTROL UNIT REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER].) (See CLIMATE CONTROL UNIT INSPECTION [FULL-AUTO AIR CONDITIONER].)
14 | A/C relay (See RELAY INSPECTION.)
15 | Blower relay (See RELAY INSPECTION.)
16 | PCM (Z6, ZJ) (See PCM INSPECTION [ZJ, Z6].)
17 | PCM (LF) (See PCM INSPECTION [LF].)
18 | PJB (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.) (See PASSENGER JUNCTION BOX (PJB) INSPECTION.)